{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["bias-tee"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"bias-tee","index":0,"n_rows":14,"n_cols":5,"rows_kept":14,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["refdes","device","value","footprint","quantity"]
["R3","potentiometer","100k","VISHAY_T18",1]
["R3","Poti-halter","100k","BI 898",1]
["R1","resistor","1k",805,1]
["R2","resistor","1k",805,1]
["R4","resistor","49R9",805,1]
["C1","capacitor","100n",805,1]
["C2","capacitor","100n",805,1]
["D1","diode","CD4148","dio_0805",1]
["L1","inductor","10u",1812,1]
["CONN1","connector","Amphenol B6252H50","BNC_LAY",1]
["CONN2","connector","Amphenol B6252H50","BNC_LAY",1]
["CONN3","connector","SMA-seitlich-an-PCB","SMA_edge",1]
["H1","mechanical","cuboid 5x10x15mm","cuboid_5x15mm",1]