{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["fixedsine_v1.1_koll"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"fixedsine_v1.1_koll","index":0,"n_rows":30,"n_cols":5,"rows_kept":30,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["refdes","footprint","value","description","qty"]
["U3","SOT89","TS78L12CY","voltage constant, 5V, 1A ",1]
["U4","SOT89","TS79L12CY","voltage constant, -5V, 1A ",1]
["CONN1","PS_3PIN_LAY","PS-3Pin","connector by JAE, IL-G series, 3 pins, model IL-G-3S-S3C2-SA",1]
["L1,L2",1812,"100uH","inductor",2]
["C11,C2",805,"1u","capacitor, SMD",2]
["U1","SOT89","TS78L05CY","voltage constant, 5V, 1A ",1]
["C12,C13,C7",805,"10n","capacitor, SMD",3]
["C10,C15,C6","tantal_7x4mm","10uF/16V","generic polarized capacitor",3]
["D2,D4,D5",1206,"CD4148","diode universal silicon",3]
["R1",805,"10k","resistor",1]
["R3",805,50,"generic resistor",1]
["L3",805,"300nH","inductor",1]
["L4",805,"750nH","inductor",1]
["C14",805,"270pF","bipolar capacitor",1]
["C16",805,"120pF","bipolar capacitor",1]
["R4",805,50,"resistor",1]
["C17",805,"1n","bipolar capacitor",1]
["R7",805,"1k","generic resistor",1]
["R2,R6",805,"1k","resistor",2]
["R5",805,"2k","resistor",1]
["C19,C21",805,"xxx","bipolar capacitor",2]
["CONN2","SMA_edge","XXX","SMA connector",1]
["U2","CRYSTEK_C32XX","unknown","Oscillator Crystek C3292xx",1]
["U5","unknown","unknown","Power pins for generic, single opamp",1]
["C18,C20,C3",805,"100n","bipolar capacitor",3]
["H1,H2,H3","M2k5_plated","hole_plated","plated hole",3]
["M1","BOX_HAMMOND_1590LLB","Hammond 1590LLB","enclosing",1]
["D1,D3","dio_1812","M6","diode, universal silicon (DUS)",2]
["C1,C4,C5,C8,C9",805,"1u","bipolar capacitor",5]