{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["interlock-KLUW_koll.bom"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":2,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"interlock-KLUW_koll.bom","index":0,"n_rows":24,"n_cols":7,"rows_kept":24,"cut":false,"hidden":false,"merged":[[23,3,23,5]],"flags":["formulas_cached_only"]}
[null,"Interlock-KLUW, v2"]
["refdes","footprint","value","description","qty","einzel €","€"]
["R9","res_RM10","2k2","resistor, through hole",1,0.02,0.02]
["R1","res_RM10","10k","resistor, through hole",3,0.02,0.06]
["R3","res_RM10","1M","resistor, wire soldered",1,0.02,0.02]
["R8","res_RM10","33k","resistor, wire soldered",1,0.02,0.02]
["R5","res_RM10","68k","resistor, wire soldered",1,0.02,0.02]
["R7","res_RM10","82k","resistor, wire soldered",1,0.02,0.02]
["R2, R6, R10","res_RM10","100k","resistor, through hole",1,0.02,0.02]
["R4","trimmer_steh_gerade","100k","trimmer, through hole",1,0.93,0.93]
["C1","cap_RM5","100n","capacitor, thru",1,0.03,0.03]
["C2","cap_RM5","1u","capacitor, SMD",1,0.17,0.17]
["D2, D3","dio_RM10","1N4001","diode universal silicon",2,0.02,0.04]
["D4","LED_3MM","LED, 20 mA","generic LED, 3mm",1,0.05,0.05]
["U1","DIP8","LM393","dual comparator",1,0.12,0.12]
["U2","TO220_LAY",7805,"voltage constant, 9V, 1A",1,0.26,0.26]
["U3","RELAY_FP2","Relay-FP2, 5V","relay AXICOM FP2, 2x Um",1,2.12,2.12]
["C3","elko_RM5_D10","100uF/16V","generic polarized capacitor",1,0.006,0.006]
["S1","APEM_TL46WW","APEM TL46WW","toggle switch, two pole",1,3.05,3.05]
["CONN1","PS_1x2PIN","PS-2","2 pin connector by JAE,  IL-G-2S-S3C2-SA",1,0.2,0.2]
["CONN2,CONN3","BNC_VERT2","BNC","BNC connector",2,3.5,7]
["M1","BOX_HAMMOND_1590B","Hammond -PSLA","enclosing",1,5.3,5.3]
[null,null,null,"Leiterplatte (1/5 von 90 €)",1,18,18]
[null,null,null,"Summe",null,null,37.456]