{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["ioboard_koll"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"ioboard_koll","index":0,"n_rows":50,"n_cols":5,"rows_kept":50,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["refdes","footprint","value","description","qty"]
["3/R1,3/R3",805,200,"generic resistor",2]
["3/R2,3/R4",805,"33k2","resistor",2]
["3/U1,3/U2","SO28W","AD976ARZ","Analog-Digital-Wandler",2]
["3/CONN1","2x20PIN_WSL_b","MPE 152-2-040-0-MTF-XS0","connector, 2 col., 40pin",1]
["5/J1,5/J2,5/J3,5/J4,5/J5,5/J6","JMP_SMD","Jumper","jumper",6]
["5/U1,5/U2","SO24W","AD7845JRZ","digital analog converter",2]
["5/CONN1","2x7PIN_WSL_b","Wannenstecker 2x7 liegend","14 pin connector, 2 columns",1]
["6/C1",805,"47pF","bipolar capacitor",1]
["6/R7",805,1200,"generic resistor",1]
["6/R2,6/R3,6/R4,6/R5,6/R6,6/R9",805,"100K","generic resistor",6]
["6/R10",805,10,"resistor",1]
["6/U1,6/U2,6/U3,6/U4","SO8","OP07","unknown",4]
["6/R8",805,68,"generic resistor",1]
["H1,H2,H3,H4,H5,H6,H7,H8","hole_M3_plated","Distanz 3mm","plated hole",8]
["4/CONN10,4/CONN11","2x20PIN_WSL_b","Wannenstecker 40-Pol","Steckverbinder 2x20PIN",2]
["4/U1,4/U2,4/U3,4/U4,4/U5","SO20","unknown","unknown",5]
["4/CONN3,4/CONN6","1x4PIN","XXX","generic 4 pin connector",2]
["4/CONN9","1x3PIN","XXX","generic three pin connector",1]
["4/S1","ALPS_EC12E","ALPS EC12E24204A9","rotational encoder",1]
["4/R7,4/R8",805,"10k","resistor",2]
["1/CONN1","MINI-FIT_JR_556_3PIN","PS-3pin","three pin DC power connector",1]
["1/C3,1/C9",805,"100nF","capacitor, SMD",2]
["1/D1,1/D2,1/D3,1/D4","dio_1210","BAV103","diode, universal silicon (DUS)",4]
["1/U3","TO220","78L12","fixed positive voltage regulator",1]
["1/U5","TO220","79L12","fixed negative voltage regulator",1]
["1/C11,1/C6","elko_RM5_D10","1000uF,16 V, Panasonic FR","generic polarized capacitor",2]
["1/L1,1/L2","ind_12x12","1000uH","inductor",2]
["1/C4,1/C8","elko_RM5_D10","1000uF,25 V","generic polarized capacitor",2]
["1/U2","SO8","OP07CD","unknown",1]
["1/U1","SO8","REF01CSZ","precision voltage reference",1]
["1/CONN2","PS_2PIN_LAY","PS_2PIN","generic 2 pin connector",1]
["1/U6","TO220","LM317T","variable positive voltage reference",1]
["1/R4",805,"XXX","resistor, SMD",1]
["1/R3",805,"330R","resistor, SMD",1]
["1/C12,3/C3","elko_RM5_D10","1000u/16V","generic polarized capacitor",2]
["1/D5,1/D6","dio_1812","M6","diode, universal silicon (DUS)",2]
["1/C13,3/C1,3/C2,3/C5,3/C6",805,"1u","bipolar capacitor",5]
["2/U4","SO8","TL081","unknown",1]
["2/C1",805,"20pF","bipolar capacitor",1]
["2/C2",805,"100nF","bipolar capacitor",1]
["1/R1,1/R2,2/R1,2/R2,2/R3,2/R5,2/R6,2/R8,2/R9,6/R1",805,"100k","generic resistor",10]
["2/CONN1_0,2/CONN2_0,2/CONN3_0,4/CONN1_0,4/CONN2_0,4/CONN4_0,4/CONN7_0,6/CONN1_0,6/CONN2_0","SMA_edge","SMA/bnc","SMA connector",9]
["2/R10",805,"100K","resistor",1]
["2/U7","SO8","LT1167","unknown",1]
["2/R12",805,500,"generic resistor",1]
["1/C1,1/C10,1/C2,1/C5,1/C7,2/C10,2/C11,2/C12,2/C13,2/C14,2/C15,2/C16,2/C3,2/C4,2/C5,2/C6,2/C7,2/C8,2/C9,3/C4,3/C8,4/C1,4/C2,4/C3,4/C4,4/C5,5/C1,5/C2,5/C3,5/C4,5/C5,5/C6,5/C7,5/C8,6/C2,6/C3,6/C4,6/C5,6/C6,6/C7,6/C8,6/C9",805,"100n","bipolar capacitor",42]
["2/U1,2/U2,2/U3,2/U5,2/U6","SO8","OP27","unknown",5]
["2/R11,2/R4,2/R7","BI_MODEL35","10k","potentiometer",3]
["2/CONN1_1,2/CONN2_1,2/CONN3_1,4/CONN1_1,4/CONN2_1,4/CONN4_1,4/CONN7_1,6/CONN1_1,6/CONN2_1","BNC_LAY","sma/BNC","BNC connector",9]