{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":6,"n_cols":4,"rows_kept":6,"cut":false,"hidden":false,"merged":[[0,0,0,3]],"flags":["formulas_cached_only"]}
["Bauteilstecker v1"]
["Bauteil","Typ","Anzahl","Beschaffung"]
["Lamellenstecker","MultiContact SA404",2,"Bürklin 12 F 160"]
["Distanzrollen","M3, 5mm",2,"Schukat KDR05"]
["Linsenkopfschraube","PH1, M3x16",2,"TME M3X16/D7985"]
["Beschriftung","Dymo D1, 12mm ","17mm","Völkner D48637"]