{"text_format":"2","workbook":"xls","n_sheets":3,"sheets":["Tabelle1","Tabelle2","Tabelle3"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":6,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Tabelle1","index":0,"n_rows":15,"n_cols":8,"rows_kept":15,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["Widerstände",null,"Kondensatoren",null,null,"Mischer"]
["2x 10 Ω",null,"1x 33 pF",null,null,"1x"]
["1x 50 Ω",null,"1x 150 pF",null,null,"DM0408LW2"]
["1x 56 Ω",null,"1x 710 pF",null,null,"Miteq"]
["1x 100 Ω"]
["1x 120 Ω",null,"Ops",null,null,"Verstärker"]
["1x 200 Ω",null,"4x CLC440",null,null,"1x"]
["1x 220 Ω",{"$nulls":4},"AMF-3B-067069-30-19P-LPN"]
["1x 240 Ω",null,"Phasendetektor",null,null,"Miteq"]
["1x 470 Ω",null,"1x"]
["1x 510 Ω",null,"MCH12140",null,null,"1x",null,"Eventuell MC100EP140"]
["1x 620 Ω",null,"ON Semiconductors",null,null,"AU-2A-0150"]
["2x 1 kΩ",{"$nulls":4},"Miteq"]
["1x 3.3 kΩ"]
["1x 100 kΩ","Poti"]

{"sheet":"Tabelle2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}

{"sheet":"Tabelle3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}