{"text_format":"2","workbook":"xls","n_sheets":4,"sheets":["Sheet1_2","Sheet1","Sheet2","Sheet3"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1_2","index":0,"n_rows":73,"n_cols":6,"rows_kept":73,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
[".START"]
["..refdes","device","value","footprint","quantity"]
["C2","POLARIZED_CAPACITOR","330uF","elko_RM5_D10",1]
["C3","POLARIZED_CAPACITOR","330uF","elko_RM5_D10",1]
["C5","POLARIZED_CAPACITOR","330uF","elko_RM5_D10",1]
["1R1","resistor","100k",805,1]
["2R1","resistor","100k",805,1]
["3R1","resistor","100k",805,1]
["4R1","resistor","100k",805,1]
["5R1","resistor","100k",805,1]
["6R1","resistor","100k",805,1]
["7R1","resistor","100k",805,1]
["8R1","resistor","100k",805,1]
["1R2","resistor","10k",805,1]
["2R2","resistor","10k",805,1]
["3R2","resistor","10k",805,1]
["4R2","resistor","10k",805,1]
["5R2","resistor","10k",805,1]
["6R2","resistor","10k",805,1]
["7R2","resistor","10k",805,1]
["8R2","resistor","10k",805,1]
["1R3","resistor","1k",805,1]
["2R3","resistor","1k",805,1]
["3R3","resistor","1k",805,1]
["4R3","resistor","1k",805,1]
["5R3","resistor","1k",805,1]
["6R3","resistor","1k",805,1]
["7R3","resistor","1k",805,1]
["8R3","resistor","1k",805,1]
["1C1","unknown","100nF",805,1]
["1C2","unknown","100nF",805,1]
["2C1","unknown","100nF",805,1]
["2C2","unknown","100nF",805,1]
["3C1","unknown","100nF",805,1]
["3C2","unknown","100nF",805,1]
["4C1","unknown","100nF",805,1]
["4C2","unknown","100nF",805,1]
["5C1","unknown","100nF",805,1]
["5C2","unknown","100nF",805,1]
["6C1","unknown","100nF",805,1]
["6C2","unknown","100nF",805,1]
["7C1","unknown","100nF",805,1]
["7C2","unknown","100nF",805,1]
["8C1","unknown","100nF",805,1]
["8C2","unknown","100nF",805,1]
["C1","unknown","100nF",805,1]
["C4","unknown","100nF",805,1]
["opampC1","unknown","100nF",805,1]
["opampC2","unknown","100nF",805,1]
["U1","unknown",7812,"TO220",1]
["U3","unknown",7912,"TO220",1]
["S1","unknown","Lorlin_CK-1049","LORLIN-CK10_1x12",1]
["U4","unknown","LT1167","SO8",1]
["1CONN1","unknown","PS-25/8G","BR","PS_1x8PIN",1]
["2CONN1","unknown","PS-25/8G","BR","PS_1x8PIN",1]
["3CONN1","unknown","PS-25/8G","BR","PS_1x8PIN",1]
["4CONN1","unknown","PS-25/8G","BR","PS_1x8PIN",1]
["5CONN1","unknown","PS-25/8G","BR","PS_1x8PIN",1]
["6CONN1","unknown","PS-25/8G","BR","PS_1x8PIN",1]
["7CONN1","unknown","PS-25/8G","BR","PS_1x8PIN",1]
["8CONN1","unknown","PS-25/8G","BR","PS_1x8PIN",1]
["CONNXLR","unknown","PS-3pin","PS_3PIN",1]
["U2","unknown","REF02","SO8",1]
["1U1","unknown","TL081","SO8",1]
["2U1","unknown","TL081","SO8",1]
["3U1","unknown","TL081","SO8",1]
["4U1","unknown","TL081","SO8",1]
["5U1","unknown","TL081","SO8",1]
["6U1","unknown","TL081","SO8",1]
["7U1","unknown","TL081","SO8",1]
["8U1","unknown","TL081","SO8",1]
["CONNBNC","unknown","XXX","BNC_VERT",1]
[".END"]

{"sheet":"Sheet1","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}

{"sheet":"Sheet2","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}

{"sheet":"Sheet3","index":3,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}